CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.6.5/conf/instr/spect/uxnmr.info
Date         : Wed Sep 27 19:57:23 2023
Release      : TopSpin 3.6.5
Installed in : C:/Bruker/TopSpin3.6.5
Host         : OKED3497
OS           : Windows 10 Pro for Workstations release 2004 (Vs 6.3)
CPU          : Intel(R) Xeon(R) W-1250 CPU @ 3.30GHz (12 cores at 3312 MHz with Hyperthreading)
User         : nmr
System       : Avance III 400 NMR spectrometer
1H-frequency : 400.13 MHz
Description  : Avance III 400
Location     : ISTB1-L2-63
Bruker Order : BH073807
Configured in: OKED3497:C:/Bruker/TopSpin3.6.5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.254
 - IPSO type: AQS
- Tctrl : 1
- Fctrls: 3
- Gctrl1: without digital preemphasis
- Rctrl : 1
- FREDs : none
- DPP : none

DRU1: AQS DRU Z100977/00687 ECL 04.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 170619
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x72   0x3    AW  R  3.0 REC-1  AQS RXAD400 Z102116/750 ECL 03.00
     3   0x34  0x2   0x1        X  5.0 REF-1  REF-400 Reference Board for AQS Receiver
     4   0x24 0x11   0x8    AE  S  2.0 SGU-1  AQS SGU/2 400 Z103080/00416 ECL 02.00 FPGA-Vs=AF
     5   0x25 0x11   0x8    AE  S  2.0 SGU-2  AQS SGU/2 400 Z103080/00415 ECL 02.00 FPGA-Vs=AF
     6   0x26 0x11   0x8    AE  S  2.7 SGU-3  AQS SGU/2 400 Z103080/03479 ECL 02.07 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  2.1 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345087_0165 W1345087/0165 ECL 2:
- TCP/IP address = 149.236.99.253
- Firmware VS    = 20120627
- Amplifier      = BLAH300 E 200-600MHZ INR: W1345087/0165 ECL 2
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/1851 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6250 ECL 50
BLA_W1345094_0097 W1345094/0097 ECL 11:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLA2X500 E 6-365MHZ INR: W1345094/0097 ECL 11
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1471 ECL 20
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/6487 ECL 50

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20220429
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 20
- Shim System = BOSS1-SB
- 2HTX Amplifier: available
- Lock: installed

Bruker Automatic Changer: device connected to 149.236.99.254:/dev/tty01
- Capacity: 60 holders
- Firmware: 20120928
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

MAS2 control unit: connected to 149.236.99.254:/dev/tty04
MAS2: device not yet configured
MAS1: device could not be configured

Eurotherm VTU: device connected to 149.236.99.254:/dev/tty05

Sample Changers at the spectrometer subnet:
-------------------------------------------------
Sample Changer 1: BACS2_H15000-01_0000
- TCP/IP address   = 149.236.99.120
- Protocol types   = SOAP

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/1 with Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H/2H 1H (virtual 50 Ohm reference: 292.5%/83.9deg)
                PN=Z003959, SN=00429 from 20070625
    Module  2 : 1H/2H 2H (virtual 50 Ohm reference: 116.1%/-72.9deg)
                PN=Z003959, SN=00429 from 20070625
    Module  3 : XBB19F 2HS
                PN=Z003504, SN=00949 from 20120411
    Module  4 : XBB19F 2HP
                PN=Z106984, SN=00013 from 20120905



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLA2X500 E 6-365MHZ INR W1345094/0097 at TCP/IP 149.236.99.252)
SGU1 AUX  output -> input 1 of transmitter 3 (BSMS 2HTX)
SGU2 NORM output -> input 1 of transmitter 1 (BLAH300 E 200-600MHZ INR W1345087/0165 at TCP/IP 149.236.99.253)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 2 of transmitter 2 (BLA2X500 E 6-365MHZ INR W1345094/0097 at TCP/IP 149.236.99.252)
SGU3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAH300 E 200-600MHZ INR W1345087/0165 at TCP/IP 149.236.99.253:
- amplifier 1H-300W uses blanking 2
- amplifier 1H-50W uses blanking 2

transmitter 2 = BLA2X500 E 6-365MHZ INR W1345094/0097 at TCP/IP 149.236.99.252:
- amplifier X-500W uses blanking 1
- amplifier X-500W uses blanking 3

transmitter 3 = BSMS 2HTX:
- amplifier 2H-20W needs no blanking


